GTwinPRO Smart card reader drivers disk for Windows 2000 Professional.
Version 1.0.0.4, October 2002.


Caution:
--------
This readme file is specifically written for the above-mentioned 
driver version. Before proceeding, you might want to check whether a
later driver version is available from www.gemplus.com


Contents:
---------

   1. Release notes
   2. Pre-Requisites
   3. Disk Content
   4. Smart Card Interface driver use
   5. User notes (Known deviations)
   6. Troubleshooting
   7. Support


1. Release notes
----------------

Version 1.0.0.4:
   This is the initial driver version certified by Microsoft.
   It is specifically designed for the 
   GKUPRO USB Kbd Smart card reader, 
   Vid=08E6 and PID=3437 with Gemcore Twin Pro chip set.


2. Pre-Requisites
-----------------

To be able to conduct the following action, you need to have
Administrator privilege on the workstation.

In the rest of this file, we assume that you know how to start the
Device Manager. To do so:
   * Right-click on the "My Computer" desktop icon and pick the
     "Properties" item in the menu.
   * Select the "Hardware" tab and click on the "Device Manager..."
     button


3. Disk Content
---------------

The following components are included with this Disk:
   - Readme.txt			V1.0
     This file.
   - GTwinUSB.Sys		V1.0
     PC/SC driver for GKUPRO
   - GTwinUSB.inf		V1.0
     Installation file for Microsoft Wizard
   - GTwinUSB.Cat
     Signature File from MS Windows Hardware Quality Labs


4. Smart Card Interface driver use
-----------------------------------

   4.1. Driver installation

      This USB device is Plug and play; you can plug it at any moment.

      4.1.1. Installation

         The first time the device is pluged, you will see a "New 
         Hardware Detected" dialog box,
         Click ,

         Select "Search for a suitable driver for your device
         (recommended)"
         Then click .

         Check the box to "Specify a location" then click .
         Browse to the driver file location (where you find this
         ReadMe.txt file) and click 
         Click  one more time to close the "Insert the 
         manufacturer's installation disk ..."
         The wizard will found a driver for the device
         Click 

         The required files are copied to your computer and the 
         device is properly configured.

         Click  to close the Hardware Wizard.


      4.1.2. Check your installation

         Right-Click on "My Computer" icon on the desktop,
         Choose "Manage" and select the "Device Manager" section,
         Double-click on "Smart Card Readers" group,
         Double-click on "USB Smart card reader"
         Select the "Driver" tab
	 Check that the "Driver version" matches the on for this file.


   4.2. Driver update

      4.2.1. Update

         Right-Click on "My Computer" icon on the desktop,
         Choose "Manage" and select the "Device Manager" section,
         Double-click on "Smart Card Readers" group,
         Double-click on "USB Smart card reader"
         Select the "Driver" tab
         Click on 

         Click , on Upgrade Driver Wizard dialog windows,
         Select "Display a list of the known drivers for this device 
         so that I can choose a specific driver", and click 
         Click 
         Browse to the driver files location (where you find this
         ReaMe.txt file) and click 
         Then click 
         Select "USB Smart card reader", and click 
         The Wizard is ready to install the driver, click .
         Click  to close the Microsoft Device Driver Wizard.

         The driver is now updated and you can close the the "USB
         Smart car reader properties" windows and "Computer 
         Management" windows.


      4.2.2. Check your update

         Right-Click on "My Computer" icon on the desktop,
         Choose "Manage" and select the "Device Manager" section,
         Double-click on "Smart Card Readers" group,
         Double-click on "USB Smart card reader"
         Select the "Driver" tab
	 Check that the "Driver version" matches the on for this file.


   4.3. Driver removal

      4.3.1. Remove

         Right-Click on "My Computer" icon on the desktop,
         Choose "Manage" and select the "Device Manager" section,
         Double-click on "Smart Card Readers" group,
         Double-click on "USB Smart card reader"
         Select the "Driver" tab
         Click on the  button.
         When prompted, confirm the operation by clicking 
         When this operation is finished, just disconnect the device.


      4.3.2. Check the removal
         
         Right-Click on "My Computer" icon on the desktop,
         Choose "Manage" and select the "Device Manager" section,
         Either no more "SmartCardReader" group appears
            no more reader is available on the computer
         Or
            Double-click on "SmartCardReader" group,
            Verify that no "USB Smart card reader" appears any
            longer.


5 - User notes (known deviations)
---------------------------------

* If you change the USB port where the reader is connected, the system
  may ask to provide source disk again! This happen only if the first
  installation was done from a removal device like floppy disk or CD.
  To resolve this issue, just copy the file on your local disk.

* After a successful uninstall, if you plug again the device, the system
  keeps traces of previous installation. If you want to remove that,
  you have to search in "%WINDIR%\inf" directory the files that begin
  with oemXX.inf and oemXX.pnf.
  Look for "USB Smart card reader" in one of those oemXX.inf.
  Then remove this file and the corresponding compiled oemxx.pnf.

6. Troubleshooting
-------------------

If the previously described procedure didn't succeed in installing or
updating the driver, please


1- To be usable, this installation requires that the Microsoft Smart Card
Manager is started.

Note: All Microsoft Smart Card Manager components are already
installed with Windows 2000.
DO NOT INSTALL THE SCBASE.EXE OR SMCLIB.EXE COMPONENTS even though
they might be part of this distribution.

To check the status of the Microsoft Smart Card Manager:
   * Start the Computer Management Console by right-clicking on the
     "My Computer" desktop icon and pick the "Manage" item in the menu,
   * Select and open the "Services and Application" group in the list,
   * Click on the "Services" item,
   * Double-click on the "Smart Card" service.
   * The service status should be "Started" and the StartUp Type should
     be "Automatic" 

If this is not the case,
   * Choose "Automatic" in the "Startup Type" drop-down list, then
   * Click on  button to start the service.

You can now close the Computer Management Console.

2- If the previously described procedure didn't succeed, please
   Open the Device Manager, 
   Click on the "Smart card readers" group and
   Check the state of the "USB Smart card reader".
   If a cross appears, or a Yellow bang "!", select the reader, 
   Click on property in the menu and 
   Check the box line "Disable in this material profile".
   Then contact the support.


7. Support
----------

In case of problem, please contact Gemplus through the Gemplus web site 
(http://www.gemplus.com/) or depending on your location :

For North America
	email : HOTLINEUSA@gemplus.com
	tel +1 (877) 436-7233

For ASIA
	email : ASIA.hotline@gemplus.com
	No phone line

For other countries
	email : hotline@gemplus.com
	tel +33 (0) 442 36 50 50

----------------------------------------------------------------------
